########################### System Information ###########################
  Windows XP Professional 5.1 Service Pack 2 (Build 2600)
  Processor info: Intel(R) Celeron(R) CPU 2.40GHz (2399MHz)
  Memory Available to Windows: 523,760 KB

############################ Program Information ###########################
  File Name: D:\Program Files\base\Alcohol Soft\Alcohol 120\Alcohol 120\Alcohol.exe
    Company Name: Alcohol Soft Development Team
    Description: Alcohol 120%
    Original: alcohol.exe
    Product: Alcohol 120%
    Trademarks: Alcohol Soft Development Team
    Copyright: Copyright(C) 2002-2005 Alcohol Soft Development Team
    Version: 1.9.5 ( Build 3105 )
    Date: 2005/07/08
    Size: 1504768 Bytes
    Hash: 8830b1347218430dfe79710699417840
    Hash(1): d1a6dcfed81ff332d01c55e3cbc5c0e68bc7c1025c3ae23577c953ca5d59955
    Hash(2): 80965b475776dcff3fc125950300bc53e7fff35f2cb2cb2f83c727ad952c740
  File Name: D:\Program Files\base\Alcohol Soft\Alcohol 120\Alcohol 120\alcoholx.dll
    Description: Alcohol virtual device control library
    Original: alcoholx.dll
    Copyright: Copyright (C) 2000-2004
    Version: 3.47.0 ( Build 0 )
    Date: 2004/08/12
    Size: 74752 Bytes
    Hash: 1b7083f2ca3a98bb3c14c3a08ad5c2d2
  File Name: D:\Program Files\base\Alcohol Soft\Alcohol 120\Alcohol 120\devsupp.dll
    Company Name: Alcohol Soft Development Team
    Description: Alcohol Software Device Capability Library
    Original: devsupp.dll
    Product: Alcohol Software Device Capability Library
    Copyright: Copyright(C) 2002-2003 Alcohol Soft Development Team
    Version: 2.4.0 ( Build 627 )
    Date: 2005/07/23
    Size: 42496 Bytes
    Hash: cb8e209009b1a3fd93103fad4efe4085

########################### User Information ###########################
  Licensed to: Happy User :)
  Registered User ID: 04EF

########################### Options Setting ###########################
  Devices control interface: Windows NT/2000/XP ATAPI/SCSI Control Interface
  CPU Priority Level: High
  Memory Buffer Size (MB): 128
  Examine the accuracy of data read from physical device: Yes
  Turn off "Auto-Select best write speed" function if possible: No
  Overburn disc(s): No
  Fill memory buffer before recording discs: Yes
  Ignore Media Type: No
  RMPS (Recordable Media Physical Signature) Emulation: No
  BAD Sectors Emulation: No
  Sub-Channel Data Fixed & Emulation: No
  Laserlock Emulation: No
  Current Language: Simplified Chinese

############################ Device(s) List ############################
  (G:) HL-DT-ST DVDRAM GSA-4120B (Port 3, Bus 0, Target 0, Lun 0)
  (H:) CDWRITER IDE5224E         (Port 3, Bus 0, Target 1, Lun 0)
  (J:) AXV CD/DVD-ROM            (Port 4, Bus 0, Target 0, Lun 0)

##################### Installed Device Drivers List #####################
  360TimeProt.sys ACPI.sys      afd.sys       agp440.sys    ALCXWDM.SYS
  AN983.sys     ATMFD.DLL     audstub.sys   Beep.SYS      BOOTVID.dll
  Cdfs.SYS      cdrom.sys     CLASSPNP.SYS  disk.sys      dmio.sys
  dmload.sys    drmk.sys      Dxapi.sys     dxg.sys       dxgthk.sys
  Fastfat.SYS   fdc.sys       Fips.SYS      flpydisk.sys  fltMgr.sys
  Fs_Rec.SYS    fsvga.sys     ftdisk.sys    gameenum.sys  hal.dll
  HIDPARSE.SYS  i8042prt.sys  imapi.sys     intelide.sys  intelppm.sys
  ipfltdrv.sys  ipsec.sys     isapnp.sys    KAVBootC.sys  kbdclass.sys
  KDCOM.DLL     KeyCrypt.sys  kmixer.sys    KNetWch.SYS   ks.sys
  KSecDD.sys    KWatch3.SYS   mnmdd.SYS     mouclass.sys  MountMgr.sys
  mrxsmb.sys    Msfs.SYS      msgpc.sys     msmpu401.sys  mssmbios.sys
  Mup.sys       MxlW2k.SYS    NDIS.sys      ndistapi.sys  ndiswan.sys
  NDProxy.SYS   netbios.sys   netbt.sys     Npfs.SYS      ntdll.dll
  Ntfs.sys      ntoskrnl.exe  Null.SYS      nv4_disp.dll  nv4_mini.sys
  nwlnkipx.sys  nwlnknb.sys   nwlnkspx.sys  parport.sys   PartMgr.sys
  pci.sys       pciide.sys    PCIIDEX.SYS   portcls.sys   psched.sys
  ptilink.sys   PxHelp20.sys  rasacd.sys    rasl2tp.sys   raspppoe.sys
  raspptp.sys   raspti.sys    rdbss.sys     RDPCDD.sys    rdpdr.sys
  redbook.sys   SCSIPORT.SYS  serenum.sys   serial.sys    swenum.sys
  sysaudio.sys  tcpip.sys     TDI.SYS       termdd.sys    update.sys
  USBD.SYS      usbehci.sys   usbhub.sys    USBPORT.SYS   usbuhci.sys
  vax347b.sys   vax347s.sys   vga.sys       VIDEOPRT.SYS  VolSnap.sys
  wanarp.sys    watchdog.sys  wdmaud.sys    win32k.sys    WMILIB.SYS    

################## Detailed Information of Device(s) ##################

  ///////////////////////////////////////////////////////////////////////
    (G:) HL-DT-ST DVDRAM GSA-4120B(3:0) detail information.
  ///////////////////////////////////////////////////////////////////////
    Vendor Identification: HL-DT-ST
    Product Identification: DVDRAM GSA-4120B
    Production Revision Level: A110
    Location: Port 3, Bus 0, Target 0, Lun 0
    Support recording method: DAO, RAW DAO(96), TAO, DVD DAO
    BURN-Free Technology: BURN-Proof
    Auto-Select best write speed: Not Supported
  -* Note: This information below is provided by the unit, it might be inaccurate. *-
  -* This software does not use this information!                                  *-
      Removable media: Yes
      Version: ATAPI (INF-8090i/INF-8020i/INF-8028i)
      Response Data Format: 02h
      CD-R Read/Write: Yes/Yes
      CD-RW Read/Write: Yes/Yes
      Read CD-R Fixed Packet: Yes
      Test Write: Yes
      DVD-ROM Read: Yes
      DVD-R Read/Write: Yes/Yes
      DVD-RAM Read/Write: Yes/Yes
      Audio Play: Yes
      Composite Audio and Video Data Stream: No
      Digital output (IEC958) on port 1 Supported: No
      Digital output (IEC958) on port 2 Supported: No
      Mode 1 Form 2: Yes
      Mode 2 Form 2: Yes
      Multi-Session: Yes
      BUF: Yes
      CD-DA Commands supported: Yes
      CD-DA Stream is Accurate: Yes
      R-W Supported: No
      R-W De-interleaved and Corrected: No
      C2 Pointers Support: Yes
      ISRC Supported: Yes
      UPC Supported: Yes
      Read Bar Code: No
      Lock media into the drive: Yes
      Currently drive Lock state: Unlocked
      Prevent Jumper: No
      Eject Command: Yes
      Separate volume levels: Yes
      Separate channel mute: Yes
      Changer Supports Disc Present: No
      Software slot selection: No
      Side change capable: No
      P through W in Lead-In: Yes

  ///////////////////////////////////////////////////////////////////////
    (H:) CDWRITER IDE5224E(3:1) detail information.
  ///////////////////////////////////////////////////////////////////////
    Vendor Identification: CDWRITER
    Product Identification: IDE5224E
    Production Revision Level: 050F
    Location: Port 3, Bus 0, Target 1, Lun 0
    Support recording method: DAO, RAW SAO, RAW SAO+SUB, RAW DAO(96), TAO
    BURN-Free Technology: Super-Link
    Auto-Select best write speed: Not Supported
  -* Note: This information below is provided by the unit, it might be inaccurate. *-
  -* This software does not use this information!                                  *-
      Removable media: Yes
      Version: ATAPI (INF-8090i/INF-8020i/INF-8028i)
      Response Data Format: 01h
      CD-R Read/Write: Yes/Yes
      CD-RW Read/Write: Yes/Yes
      Read CD-R Fixed Packet: Yes
      Test Write: Yes
      DVD-ROM Read: No
      DVD-R Read/Write: No/No
      DVD-RAM Read/Write: No/No
      Audio Play: Yes
      Composite Audio and Video Data Stream: No
      Digital output (IEC958) on port 1 Supported: No
      Digital output (IEC958) on port 2 Supported: No
      Mode 1 Form 2: Yes
      Mode 2 Form 2: Yes
      Multi-Session: Yes
      BUF: Yes
      CD-DA Commands supported: Yes
      CD-DA Stream is Accurate: Yes
      R-W Supported: No
      R-W De-interleaved and Corrected: No
      C2 Pointers Support: Yes
      ISRC Supported: Yes
      UPC Supported: Yes
      Read Bar Code: No
      Lock media into the drive: Yes
      Currently drive Lock state: Unlocked
      Prevent Jumper: No
      Eject Command: Yes
      Separate volume levels: Yes
      Separate channel mute: Yes
      Changer Supports Disc Present: No
      Software slot selection: No
      Side change capable: No
      P through W in Lead-In: Yes

#######################################################################

###################### Source Disc/Image Information ######################
类型: 	标准 ISO 镜像
路径: 	D:\Downloads\MIDI工具\Adobe Photoshop CS2 v9.0 简体中文正式光盘版\
名称: 	Adobe.Photoshop.CS2.V9.0.简体中文正式光盘版.PhotoshopCS2_CHS.iso 
大小:	279.15 MB
区段:	1
轨道:	1


区段 01: 
  轨道 01: Mode 1, 长度: 142926(279.2 MB), 地址: 000000
#############################################################################

####################### Dumping/Recording Progress Log #######################
00:06:44 处理器信息:Intel(R) Celeron(R) CPU 2.40GHz (2399MHz)
00:06:44 可用内存:523,760 KB
00:06:44 缓存大小:128 MB
00:06:45 载入镜像文件中: D:\Downloads\MIDI工具\Adobe Photoshop CS2 v9.0 简体中文正式光盘版\Adobe.Photoshop.CS2.V9.0.简体中文正式光盘版.PhotoshopCS2_CHS.iso
00:06:45 来源信息: 区段: 1, 轨道: 1, 长度: 279.2 MB / 031:45:51
00:06:50 (G:) HL-DT-ST DVDRAM GSA-4120B(3:0): 烧录模式/速度
00:06:50 烧录中 - DAO / SAO - 40X (6000 KB/秒)
00:06:50 (G:) HL-DT-ST DVDRAM GSA-4120B(3:0): 已激活 BURN-Free 功能
00:08:12 镜像文件载入完毕!
00:08:46 (G:) HL-DT-ST DVDRAM GSA-4120B(3:0): 烧录成功完成!
00:08:46 逝去时间: 00:01:55, 平均速度: 18.1X
##############################################################################

