########################### System Information ###########################
  Windows XP Professional 5.1 Service Pack 2 (Build 2600)
  Processor info: Intel(R) Celeron(R) CPU 2.40GHz (2399MHz)
  Memory Available to Windows: 523,760 KB

############################ Program Information ###########################
  File Name: D:\Program Files\base\Alcohol Soft\Alcohol 120\Alcohol.exe
    Company Name: Alcohol Soft Development Team
    Description: Alcohol 120%
    Original: alcohol.exe
    Product: Alcohol 120%
    Trademarks: Alcohol Soft Development Team
    Copyright: Copyright(C) 2002-2006 Alcohol Soft Development Team
    Version: 1.9.5 ( Build 4212 )
    Date: 2006/06/13
    Size: 4354432 Bytes
    Hash: 0b6923f6c130958848cc781f618b77c0
    Hash(1): d1a71e678f2ffa4f3412ca3b735f9f7d92bcd2cbb987599324c94768d5816c0ff9
    Hash(2): 996873f476e259affc0d0951d3276e4bb713b395e6b51de3d1d665d6e7e72a5900
  File Name: D:\Program Files\base\Alcohol Soft\Alcohol 120\alcoholx.dll
    Company Name: Alcohol Soft Co., Ltd.
    Description: Alcohol virtual device control library
    Original: alcoholx.dll
    Product: Alcohol
    Copyright: Copyright (C) 2000-2006
    Version: 4.3.0 ( Build 0 )
    Date: 2006/01/25
    Size: 403352 Bytes
    Hash: 8c1efe717203eed1b9f91da81083ba1c
  File Name: D:\Program Files\base\Alcohol Soft\Alcohol 120\devsupp.dll
    Company Name: Alcohol Soft Development Team
    Description: Alcohol Software Device Capability Library
    Original: devsupp.dll
    Product: Alcohol Software Device Capability Library
    Copyright: Copyright(C) 2002-2006 Alcohol Soft Development Team
    Version: 2.5.1 ( Build 1813 )
    Date: 2006/06/13
    Size: 46592 Bytes
    Hash: d5bfa4f189153243c7cc1f16b647b32e

########################### User Information ###########################
  Licensed to: RL-Team.NeT
  Registered User ID: 1000

########################### Options Setting ###########################
  Devices control interface: Windows NT/2000/XP ATAPI/SCSI Control Interface
  CPU Priority Level: High
  Memory Buffer Size (MB): 128
  Examine the accuracy of data read from physical device: Yes
  Turn off "Auto-Select best write speed" function if possible: No
  Overburn disc(s): No
  Fill memory buffer before recording discs: Yes
  Virtual Device Sub-System: *** Not avaliable ***
  Current Language: Simplified Chinese

############################ Device(s) List ############################
  (G:) HL-DT-ST DVDRAM GSA-4120B (Port 3, Bus 0, Target 0, Lun 0)
  (H:) CDWRITER IDE5224E         (Port 3, Bus 0, Target 1, Lun 0)

##################### Installed Device Drivers List #####################
  ACPI.sys      afamgt.sys    afd.sys       agp440.sys    ALCXWDM.SYS
  AmdPci32.sys  AN983.sys     atapi.sys     ATMFD.DLL     BATTC.SYS
  bb-run.sys    Beep.SYS      BOOTVID.dll   cda1000.sys   Cdfs.SYS
  cdrom.sys     CLASSPNP.SYS  compbatt.sys  disk.sys      dmio.sys
  dmload.sys    DontGo.sys    drmk.sys      Dxapi.sys     dxg.sys
  dxgthk.sys    Fastfat.sys   fdc.sys       Fips.SYS      fltMgr.sys
  Fs_Rec.SYS    fsvga.sys     ftdisk.sys    gameenum.sys  hal.dll
  HTTP.sys      i2omgmt.SYS   i8042prt.sys  imapi.sys     intelide.sys
  intelppm.sys  ipfltdrv.sys  ipnat.sys     ipsec.sys     isapnp.sys
  JGOGO.sys     KAVBase.sys   KAVBootC.sys  kbdclass.sys  KDCOM.DLL
  kmixer.sys    KNetWch.SYS   ks.sys        KSecDD.sys    KWatch3.SYS
  mnmdd.SYS     mouclass.sys  MountMgr.sys  mrxdav.sys    mrxsmb.sys
  Msfs.SYS      msgpc.sys     msmpu401.sys  Mup.sys       NDIS.sys
  ndistapi.sys  ndisuio.sys   ndiswan.sys   NDProxy.SYS   netbios.sys
  netbt.sys     Npfs.SYS      ntdll.dll     ntoskrnl.exe  ntoskrnl.exe
  Null.SYS      nv4_disp.dll  nv4_mini.sys  nwlnkflt.sys  nwlnkfwd.sys
  nwlnkipx.sys  nwlnknb.sys   nwlnkspx.sys  parport.sys   PartMgr.sys
  pci.sys       PCIIDEX.SYS   portcls.sys   psched.sys    ptilink.sys
  PxHelp20.sys  rasacd.sys    rasl2tp.sys   raspppoe.sys  raspptp.sys
  raspti.sys    rdbss.sys     RDPCDD.sys    redbook.sys   SCSIPORT.SYS
  SENTINEL.SYS  serenum.sys   serial.sys    SiRemFil.sys  SiWinAcc.sys
  srv.sys       swenum.sys    sysaudio.sys  tcpip.sys     TDI.SYS
  termdd.sys    USBD.SYS      usbehci.sys   usbhub.sys    USBPORT.SYS
  usbuhci.sys   vga.sys       VIDEOPRT.SYS  vmscsi.sys    VolSnap.sys
  wanarp.sys    watchdog.sys  wdmaud.sys    win32k.sys    WMILIB.SYS
  xfilt.sys     

################## Detailed Information of Device(s) ##################

  ///////////////////////////////////////////////////////////////////////
    (G:) HL-DT-ST DVDRAM GSA-4120B(3:0) detail information.
  ///////////////////////////////////////////////////////////////////////
    Vendor Identification: HL-DT-ST
    Product Identification: DVDRAM GSA-4120B
    Production Revision Level: A110
    Location: Port 3, Bus 0, Target 0, Lun 0
    Support recording method: DAO, RAW SAO, RAW SAO+SUB, RAW DAO(96), TAO, DVD DAO
    BURN-Free Technology: Super-Link
    Auto-Select best write speed: Not Supported
  -* Note: This information below is provided by the unit, it might be inaccurate. *-
  -* This software does not use this information!                                  *-
      Removable media: Yes
      Version: ATAPI (INF-8090i/INF-8020i/INF-8028i)
      Response Data Format: 02h
      CD-R Read/Write: Yes/Yes
      CD-RW Read/Write: Yes/Yes
      Read CD-R Fixed Packet: Yes
      Test Write: Yes
      DVD-ROM Read: Yes
      DVD-R Read/Write: Yes/Yes
      DVD-RAM Read/Write: Yes/Yes
      Audio Play: Yes
      Composite Audio and Video Data Stream: No
      Digital output (IEC958) on port 1 Supported: No
      Digital output (IEC958) on port 2 Supported: No
      Mode 1 Form 2: Yes
      Mode 2 Form 2: Yes
      Multi-Session: Yes
      BUF: Yes
      CD-DA Commands supported: Yes
      CD-DA Stream is Accurate: Yes
      R-W Supported: No
      R-W De-interleaved and Corrected: No
      C2 Pointers Support: Yes
      ISRC Supported: Yes
      UPC Supported: Yes
      Read Bar Code: No
      Lock media into the drive: Yes
      Currently drive Lock state: Unlocked
      Prevent Jumper: No
      Eject Command: Yes
      Separate volume levels: Yes
      Separate channel mute: Yes
      Changer Supports Disc Present: No
      Software slot selection: No
      Side change capable: No
      P through W in Lead-In: Yes

  ///////////////////////////////////////////////////////////////////////
    (H:) CDWRITER IDE5224E(3:1) detail information.
  ///////////////////////////////////////////////////////////////////////
    Vendor Identification: CDWRITER
    Product Identification: IDE5224E
    Production Revision Level: 050F
    Location: Port 3, Bus 0, Target 1, Lun 0
    Support recording method: DAO, RAW SAO, RAW SAO+SUB, RAW DAO(96), TAO
    BURN-Free Technology: Super-Link
    Auto-Select best write speed: Not Supported
  -* Note: This information below is provided by the unit, it might be inaccurate. *-
  -* This software does not use this information!                                  *-
      Removable media: Yes
      Version: ATAPI (INF-8090i/INF-8020i/INF-8028i)
      Response Data Format: 01h
      CD-R Read/Write: Yes/Yes
      CD-RW Read/Write: Yes/Yes
      Read CD-R Fixed Packet: Yes
      Test Write: Yes
      DVD-ROM Read: No
      DVD-R Read/Write: No/No
      DVD-RAM Read/Write: No/No
      Audio Play: Yes
      Composite Audio and Video Data Stream: No
      Digital output (IEC958) on port 1 Supported: No
      Digital output (IEC958) on port 2 Supported: No
      Mode 1 Form 2: Yes
      Mode 2 Form 2: Yes
      Multi-Session: Yes
      BUF: Yes
      CD-DA Commands supported: Yes
      CD-DA Stream is Accurate: Yes
      R-W Supported: No
      R-W De-interleaved and Corrected: No
      C2 Pointers Support: Yes
      ISRC Supported: Yes
      UPC Supported: Yes
      Read Bar Code: No
      Lock media into the drive: Yes
      Currently drive Lock state: Unlocked
      Prevent Jumper: No
      Eject Command: Yes
      Separate volume levels: Yes
      Separate channel mute: Yes
      Changer Supports Disc Present: No
      Software slot selection: No
      Side change capable: No
      P through W in Lead-In: Yes

#######################################################################

###################### Source Disc/Image Information ######################
类型: 	标准 ISO 镜像
路径: 	E:\game\Cs1.6中文版\Cs1.6中文版\新建文件夹\[2007-12-18]猪猪猫.CN-WINXPSP2电脑城装机12[标准版]\猪猪猫.CN-WINXPSP2电脑城装机12标准版\
名称: 	猪猪猫.CN-WINXPSP2电脑城装机12标准版.iso 
大小:	681.97 MB
区段:	1
轨道:	1


区段 01: 
  轨道 01: Mode 1, 长度: 349170(682.0 MB), 地址: 000000
#############################################################################

####################### Dumping/Recording Progress Log #######################
********* Time stamp of this log file:  2008-01-01 15:06:30 *********
15:06:30 处理器信息:Intel(R) Celeron(R) CPU 2.40GHz (2399MHz)
15:06:30 可用内存:523,760 KB
15:06:30 系统内存不足, 自动调整缓存到 93 MB.
15:06:30 载入镜像文件中: E:\game\Cs1.6中文版\Cs1.6中文版\新建文件夹\[2007-12-18]猪猪猫.CN-WINXPSP2电脑城装机12[标准版]\猪猪猫.CN-WINXPSP2电脑城装机12标准版\猪猪猫.CN-WINXPSP2电脑城装机12标准版.iso
15:06:30 来源信息: 区段: 1, 轨道: 1, 长度: 682.0 MB / 077:35:45
15:06:33 (G:) HL-DT-ST DVDRAM GSA-4120B(3:0): 烧录模式/速度
15:06:33 烧录中 - DAO / SAO - 10X (1500 KB/秒)
15:06:33 (G:) HL-DT-ST DVDRAM GSA-4120B(3:0): 已激活 BURN-Free 功能
15:14:08 镜像文件载入完毕!
15:15:11 (G:) HL-DT-ST DVDRAM GSA-4120B(3:0): 烧录成功完成!
15:15:11 逝去时间: 00:08:37, 平均速度: 9.4X
##############################################################################

